# show ip rpf-route

#### Syntax

show ip rpf-route [ vrf vrfName ] [ destination [ ipMask ] [ detail ] ]
[ all ] [ protocol ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays routes that the router can use to verify source addresses in multicast packets.

#### Options

- vrfName—Displays the contents of the IP routing table associated with a VRF
- destination—Specifies the IP address or domain name of the host to show
- ipMask—IP mask of the specific address to show
- detail—Displays detailed information about the specific prefix; currently shows the tag added by means of the ip route command
- all—Displays all routes in the routing table inserted from all protocols (not just the best routes that are used for forwarding)
- protocol—One of the following protocols for which you want to display the best routes in the routing table; no routes are displayed if routes for the specified protocol are not present in the routing table
  - access—Displays the best access-server routes (BGP) in the routing table
  - access-internal—Displays the best access-internal routes in the routing table
  - bgp—Displays the best BGP routes in the routing table
  - bgp-tunnel—Displays the best BGP tunnel routes in the routing table
  - dvmrp—Displays the best DVMRP routes in the routing table
  - isis—Displays the best IS-IS routes in the routing table
  - ldp—Displays the best LDP tunnel routes in the routing table
  - local—Displays the best locally connected routes in the routing table
  - mbgp—Displays the best MBGP routes in the routing table
  - ospf—Displays the best OSPF routes owned by in the routing table
  - other—Displays the best internal control routes in the routing table
  - rip—Displays the best RIP routes in the routing table
  - rsvp—Displays the best RSVP tunnel routes in the routing table
  - static—Displays the best static routes added by network management to the routing table
  - static-rpf—Displays the best static RPF routes added by network management to the routing table
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec