# ipv6 access-route table-map

#### Syntax

ipv6 access-route [ vrf vrfName ] table-map mapName

no ipv6 access-route [ vrf vrfName ] table-map [ mapName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Filters access routes before an access list adds them to the routing table. The no version deletes the table map.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- mapName—Name of the table map that you want the router to use

#### Mode

Global Configuration