# aaa subscriber limit per-vr

#### Syntax

aaa subscriber limit per-vr limitValue

no aaa subscriber limit per-vr

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the maximum number of active subscribers permitted on the virtual router. The no version returns the limit to the default, 0 (zero).

#### Options

- limitValue—Maximum number of subscribers; default value is 0 (zero), which means there is no limit on the number of subscribers

#### Mode

Global Configuration