# path ds3 shutdown

#### Syntax

[ no ] path pathChannel ds3 ds3Channel shutdown

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Disables a DS3 signal. This command applies to a DS3 over channelized SONET interface. DS3 interfaces are enabled by default. The no version restarts a disabled interface.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the path

#### Mode

Controller Configuration