Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Setting a Statistics Baseline for Policies

# atm policy

#### Syntax

atm policy { input | output } policyName
[ statistics { enabled [ preserve | merge ] | disabled [ merge ] } | merge ]

no atm policy { input | output } [ policyName ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
merge keyword added in JunosE Release 7.2.0.

#### Description

Assigns a policy list to the ingress or egress of an ATM interface. If you enter this command when the policy list does not exist, the router creates a policy list with a filter rule as the default. You must specify the input or output keyword to assign the policy list to the ingress or egress of the interface. The no version removes the association between a policy list and an interface.

#### Options

- input—Applies policy to data arriving at this interface
- output—Applies policy to data leaving this interface
- policyName—Name of the policy; a maximum of 40 characters
- statistics—Enables or disables collection of policy routing statistics
  - enabled—Enables collection of policy routing statistics
  - preserve—Preserves existing statistics for any classifier-list that is the same for both the new and old policy attachments when you attach a new policy to an interface
  - disabled—Disables collection of policy routing statistics
- merge—Enables merging of multiple policies to form a single policy

#### Mode

Interface Configuration

## Related Documentation

- Setting a Statistics Baseline for Policies

#### Published: 2011-04-07

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out