# radius per-profile-attr-list

#### Syntax

[ no ] radius per-profile-attr-list profileName

#### Release Information

Command introduced in JunosE Release 12.1.0.

#### Description

Creates a new RADIUS per-profile attribute list and puts the E Series router into RADIUS-Profile Configuration mode. The no version removes the configured RADIUS per-profile attribute list. By default, no attribute list is configured.

#### Options

- profileName—Name of the RADIUS per-profile; string of up to 32 characters

#### Mode

Global Configuration

#### Related Documentation

- Configuring a Per-Profile RADIUS Attribute List in the JunosE Broadband Access Configuration Guide
- radius include