# baseline mpls next-hop

#### Syntax

baseline mpls next-hop nextHopIndex

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for the specified MPLS next hop. Statistics for a next hop must be enabled with the mpls statistics next-hop command before they can be baselined. By default, the next-hop counters are baselined at zero. There is no no version.

#### Options

- nextHopIndex—Number identifying a next hop; displayed by the show mpls forwarding command

#### Mode

Privileged Exec