# ip flow-cache timeout

#### Syntax

ip flow-cache timeout { active activeTimer | inactive inactiveTimer }

no ip flow-cache timeout { active | inactive }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines the J-Flow activity or inactivity timers. The no version restores the default value of each timer.

#### Options

- activeTimer—Value of activity timer in the range 0–60 minutes; default value is 30
- inactiveTimer—Value of inactivity timer in the range 10–600 seconds; default value is 15

#### Mode

Global Configuration