# show icr-partition

#### Syntax

show icr-partition [ interfaceType interfaceSpecifier [ vrid ] ] [ filter ]

#### Release Information

Command introduced in JunosE Release 10.3.0.

#### Description

Displays ICR partition information for the VRID configured on the specified interface.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - fastEthernet
  - gigabitEthernet
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- vrid—Virtual router ID identifier; a number in the range 1– 255
- filter—See Filtering show Commands

#### Mode

Privileged Exec

#### Related Documentation

- Monitoring the Configuration of an ICR Partition Attached to an Interface
- Monitoring the Status of ICR Partition Accounting
- Monitoring the Configuration of ICR Partitions