# l2c end-user-id

#### Syntax

l2c end-user-id idString neighbor neighborName

no l2c end-user-id idString

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates the GSMP output label associated with the interface. In addition to the label, this command also specifies the access node using the neighbor keyword. The no version removes the output label association.

#### Options

- idString—String to identify the GSMP label
- neighborName—Name of the neighboring access node

#### Mode

Interface Configuration, Subinterface Configuration