# snmp-server community

#### Syntax

snmp-server community commString [ view viewName ] [ priv ] [ accessListName ]

no snmp-server community commString

#### Release Information

Command introduced before JunosE Release 7.1.0.
view keyword and viewName variable added in JunosE Release 7.1.0.

#### Description

Configures an authorized SNMP community and associates SNMPv1/v2c communities with SNMPv3 views. The no version removes an authorized community from the list of communities.

#### Options

- commString—Name of the SNMPv1/v2c community
- viewName—Name of the SNMPv3 view, which allows configuration using available dynamic views
- priv—Privileged Exec level: ro (read-only), rw (read-write), or admin (administrator)
- accessListName—Name of IP access list to filter SNMP clients

#### Mode

Global Configuration