# Using RADIUS to Manage Subscribers Logging In to ICR Partitions

To configure RADIUS to manage subscribers logging in to ICR partitions on the router, perform the following tasks:

- Configure inclusion of the ICR-Partition-ID VSA in RADIUS messages.
  host1(config)#radius-include icr-partition-id acct-start enable

  Issuing this command includes the ICR-Partition-ID VSA in Acct-Start messages. To include the ICR-Partition-ID VSA in other accounting and access messages, see the Configuring RADIUS Attributes chapter in the JunosE Broadband Access Configuration Guide.

- Enable or disable sending of the ICR Partition-Accounting-On or Partition-Accounting-Off messages to the RADIUS servers.
  host1(config)#radius icr-partition-accounting enable

  For more information on enabling or disabling sending of partition accounting messages to RADIUS servers configured on a virtual router, see the Configuring RADIUS Attributes chapter in the JunosE Broadband Access Configuration Guide.

#### Related Documentation

- Interaction with RADIUS for ICR
- Configuring an ICR Partition
- radius include
- radius icr-partition-accounting
- show radius icr-partition-accounting