Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring Traffic Classes That Define Service Levels
- show traffic-class

# Monitoring Service Levels with Traffic Classes

#### Purpose

Display information about traffic classes.

#### Action

To display information about all traffic classes:

    host1#show traffic-class
                           fabric
    traffic       fabric   strict
    class         weight   priority
    -----------   ------   --------
    best-effort     8         no
    best-effort     8         no
    tc1             8         no
    tc2             8         no
    tc3             8         no
    tcs4            8        yes
    tcs5            8        yes

To display the number of times that a QoS profile references the traffic class:

    host1#show traffic-class brief
    traffic-class best-effort referenced 17 times in qos-profiles

To display a list of QoS profiles and traffic-class groups that reference the traffic class:

    host1#show traffic-class references
    traffic-class best-effort
      Referenced by QoS profiles:
        atm-default
        serial-default
        ethernet-default
        server-default
      Referenced by traffic class groups:
        None

#### Meaning

Table 1 lists the show traffic-class command output fields.

Table 1: show traffic-class Output Fields

Field Name | Field Description
--- | ---
traffic class | Name of the traffic class
fabric weight | Weight of the queue in the fabric
fabric strict priority | Setting strict-priority queues in the fabric
Referenced by QoS profiles | QoS profiles that reference this traffic class
Referenced by traffic class groups | Traffic-class groups that reference this traffic class

## Related Documentation

- Configuring Traffic Classes That Define Service Levels
- show traffic-class

#### Published: 2011-03-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out