Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Creating a Classifier Group for a Policy List
- Configuring CLI-Based Mirroring

# classifier-group

#### Syntax

classifier-group { * | classifierName } [ precedence precValue ] [ parent-group parentGroupName ] [ external parent-group externalParentGroupName
parameter parameterName ]

no classifier-group { * | classifierName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
parent-group keyword and parentGroupName variable added in JunosE Release 7.2.0.
external parent-group keyword and externalParentGroupName variable added in JunosE Release 8.0.0.

#### Description

Creates a classifier group for a policy list and assigns precedence to the specific CLACL in the group. This command accesses Classifier Group Configuration mode, in which you create policy rule configurations related to the specified CLACL. If a parent group was not created by the parent-group command, the parent-group keyword creates a parent group in a rate-limit hierarchy for IP, IPv6, L2TP, and MPLS. All packets matching the classifier are sent to the parent group for further processing, except for packets dropped by the classifier using the filter rule. More than one classifier group can have the same parent group, which enables you to create hierarchies. The no version removes the classifier group and its rules from the policy list.

#### Options

- *—Specifies that the router selects all packets from the interface associated with the policy list for this classifier group
- classifierName—Name of a specific CLACL used to classify packets in this policy list
- precValue—Precedence value for the CLACL, in the range 0–65535; a value of 100 is assigned if no value is specified
- parentGroupName—Name of the parent group; if the parent group does not exist, naming the parent group creates an empty parent group

  | Note: Secure policy lists, which are used for packet mirroring operations, do not support named classifier groups. You must use classifier-group *. Also, secure policy lists do not support the precedence keyword.

- externalParentGroupName—External parent group name
- parameterName—Parameter name

#### Mode

Policy List Configuration

## Related Documentation

- Creating a Classifier Group for a Policy List
- Configuring CLI-Based Mirroring

#### Published: 2011-04-07

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out