Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring Interface Sets for QoS
- show qos-interface-set

# Monitoring the Configuration of QoS Interface Sets

#### Purpose

Display information about configured interface sets.

#### Action

To display information about a specific interface set:

    host1#show qos-interface-set vlan-set
    interface                  member member restricted
       set    parent   port     type  count  interface
    --------- ------ --------- ------ ------ ----------
    vlan-set  vlan-ss lag test1 vlan   2        none

To display detailed information about a specific interface set:

    host1#show qos-interface-set vlan-set detail
    interface                   member member restricted
       set    parent    port     type  count  interface
    --------- ------- --------- ------ ------ ----------
    vlan-set  vlan-ss lag test1  vlan    2      none

    Children:
      vlan lag test1.1      vlan lag test1.4

#### Meaning

Table 1 lists the show qos-interface-set command output fields.

Table 1: show qos-interface-set Output Fields

Field Name | Field Description
--- | ---
interface set | Name of the interface set
parent | Name of the interface superset that is the parent of the interface set
port | Interface that is the parent of the interface superset
member type | Member-interface type defined for the interface set: vlan ip vlan
restricted interface | Restricted interface configured for this interface set
Children | List of interface members associated with the interface superset

## Related Documentation

- Configuring Interface Sets for QoS
- show qos-interface-set

#### Published: 2011-03-17

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out