# clear ip mroute

#### Syntax

clear ip mroute { * | grpAddress [ sourceAddress ] }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Clears all or the specified multicast forwarding entries. There is no no version.

#### Options

- *—Clears all IP multicast forwarding entries
- grpAddress—Address of the multicast group for which forwarding entries should be cleared
- sourceAddress—Address of the multicast source for which forwarding entries should be cleared

#### Mode

Privileged Exec, User Exec