# show ipv6 pim sparse-mode unicast-route

#### Syntax

show ipv6 pim sparse-mode unicast-route [ routeAddress routeMask | ipv6Prefix ]
[ count ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays the IPv6 unicast routes that PIM sparse mode is using.

#### Options

- routeAddress—IPv6 address associated with a unicast route
- routeMask—Network mask associated with a unicast route
- ipv6Prefix—Prefix in the format IPv6BaseAddress / length; for example, 1::1/32
- count—Shows the number of unicast routes that PIM sparse mode is using
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec