# Establishing the IGMP Proxy Baseline

You can set the counters for the number of queries received and reports sent on the upstream interface to zero. This feature enables you to establish a reference point, or baseline, for IGMP proxy statistics.

baseline ip igmp-proxy interface

- Use to set the counters for the number of queries received and reports sent on the upstream interface to zero.

  | Note: Issue this command only on the upstream interface. Otherwise, this command has no effect.

- Example
  (host1)#baseline ip igmp-proxy interface
- There is no no version.
- See baseline ip igmp-proxy interface.