# radius calling-station-delimiter

#### Syntax

radius calling-station-delimiter delimiter

no radius calling-station-delimiter

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the delimiter for DSL PPP users for RADIUS attribute 31, Calling-Station-Id. The no version removes the delimiter.

#### Options

- delimiter—Special character to set off items in the Calling-Station-Id’s definition (for example, # or %)

#### Mode

Global Configuration