# path ds3

#### Syntax

path pathChannel ds3 ds3Channel { [ channelized ] | unchannelized }

no path pathChannel ds3 ds3Channel

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates and configures a DS3 signal. This command applies to a DS3 over channelized SONET interface. If you do not specify whether or not the path should be channelized, the router creates a channelized path by default. The no version deletes a path.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the path

#### Mode

Controller Configuration