# aps group

#### Syntax

aps group groupName

no aps group

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns an interface to an APS/MSP group. The no version removes a group of APS/MSP interfaces.

#### Options

- groupName—Name of the APS/MSP group to which the active and standby interfaces belong; string of up to 32 characters

#### Mode

Controller Configuration