# aaa accounting statistics

#### Syntax

aaa accounting statistics { volume-time | time }

no aaa accounting statistics

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Configures the router to collect either a full set of statistics or only uptime status for the sessions AAA is managing. Collecting only the uptime status is a more efficient use of system resources. The no version restores the default setting in which the router collects full statistics.

#### Options

- volume-time—Collects a full complement of statistics from each connection; the default setting
- time—Collects only uptime status for each connection

#### Mode

Global Configuration