# show l2tp dial-out virtual-router

#### Syntax

show l2tp dial-out virtual-router [ allVirtualRouters ] [ detail ] [ state operState ]
[ filter ]

To display summary information:

show l2tp dial-out virtual-router summary [ allVirtualRouters ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays dial-out state machine operational status and statistics within the current virtual router context.

#### Options

- allVirtualRouters—Displays dial-out information across all virtual routers
- detail—Displays configuration, state, and statistics
- operState—One of the following operational states:
  - down
  - inService
  - initFailed
  - initPending
- filter—See Filtering show Commands
- summary—Displays aggregate counts for dial-out state machines in each of the possible operational and administrative states

#### Mode

Privileged Exec