# show radius nas-port-format extended

#### Syntax

show radius nas-port-format extended { atm | ethernet } [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Displays the format used for RADIUS attribute 5, NAS-Port, on the E120 router and the E320 router.

#### Options

- atm—Displays information about ATM interfaces
- ethernet—Displays information about Gigabit Ethernet and 10-Gigabit Ethernet interfaces
- filter—See Filtering show Commands

#### Mode

Privileged Exec