# global export map

#### Syntax

global export map [ ipv4 | ipv6 ] routeMap

no global export map [ ipv4 | ipv6 ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Associates a route map with a VRF to modify and filter routes exported by the VRF to the global BGP non-VPN RIB in the parent VR. Both IPv4 and IPv6 routes are exported unless you issue the appropriate keyword to restrict exportation. The no version disables the exporting of routes to the global BGP non-VPN RIB.

#### Options

- ipv4—Specifies that only IPv4 routes are exported to the global BGP non-VPN RIB
- ipv6—Specifies that only IPv6 routes are exported to the global BGP non-VPN RIB
- routeMap—Name of a route map; string of up to 32 alphanumeric characters

#### Mode

VRF Configuration