# baseline ip dhcp-external

#### Syntax

baseline ip dhcp-external

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a baseline for DHCP external server statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Mode

Privileged Exec

#### Related Documentation

- Setting Baselines for DHCP Statistics