# ppp ipcp netmask

#### Syntax

[ no ] ppp ipcp netmask

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Explicitly enables the IPCP option 0x90 on a per-PPP interface basis, either in a profile or on a static interface. By default, the IPCP option 0x90 is disabled on the interface. The no version disables the IPCP option 0x90.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration