# show ipv6 static

#### Syntax

show ipv6 static [ vrf vrfName ] [ ipv6Prefix [ all ] ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Displays general status information for static routes added by network management to the routing table.

#### Options

- vrfName—Name of the VRF
- ipv6Prefix—Prefix in the format IPv6baseaddress / length; for example, 1::1/32
- all—Displays all routes starting at the specified prefix
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec