# mpls ldp ip-forwarding

#### Syntax

[ no ] mpls ldp ip-forwarding [ { access-list | prefix-list } listName ) ] [ host-only ]

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Specifies LSPs to be put into the IP routing table for forwarding plain IP traffic. The no version removes the listed LSPs or all LSPs from the IP routing table.

| Note: This command replaces the deprecated mpls topology-driven-lsp ip-interfaces command.

| Note: Although the carriage return, <cr>, option is displayed when you type a question mark (?) after entering the mpls ldp ip-forwarding command, this command takes effect only if the access-list, host-only, or prefix-list keyword, or a combination of them is specified. Otherwise, although the command is configured successfully and no error is displayed, labels are not used in the IP routing table for forwarding plain IP traffic. This behavior for this command began in JunosE Release 7.1.0, in which the command was introduced.

#### Options

- access-list—Specifies that listName is an access list
- prefix-list—Specifies that listName is a prefix list
- listName—Name of access list or prefix list that specifies LSPs over which IP interfaces are created
- host-only—Specifies that IP interfaces are created only over LSPs to host addresses

#### Mode

Global Configuration