# Monitoring Local Address Pools

#### Purpose

Display information about the local address pools configured on your router. If you do not specify the name of a local address pool, the router displays all local address pools.

#### Action

To display information about local address pools:

    host1#show ip local pool

             High    Abated
    Pool    Thresh   Thresh   Trap   Group
    -----   ------   ------   ----   -----
    poolA       85       75    N

         Aliases
         -------
          alias1
                                       In
          Begin        End      Free   Use
         --------   ---------   ----   ---
         10.1.1.1   10.1.1.10    10     0
         10.1.2.1   10.1.2.10    10     0
         10.1.3.1   10.1.3.10    10     0

             High    Abated
    Pool    Thresh   Thresh   Trap   Group
    -----   ------   ------   ----   -----
    poolB       85       75    N

         Aliases
         -------
          alias2
                                       In
          Begin        End      Free   Use
         --------   ---------   ----   ---
         10.2.1.1   10.2.1.10    10     0
         10.2.2.1   10.2.2.10    10     0

             High    Abated
    Pool    Thresh   Thresh   Trap   Group
    -----   ------   ------   ----   -----
    poolC       85       75    N

         Aliases
         -------
          alias3
                                       In
          Begin        End      Free   Use
         --------   ---------   ----   ---
         10.3.1.1   10.3.1.10    10     0

             High    Abated
    Pool    Thresh   Thresh   Trap   Group
    -----   ------   ------   ----   -----
    poolD       85       75    N

         Aliases
         -------
           poolA
           poolB
           poolC
                                        In
          Begin        End       Free   Use
         --------   ----------   ----   ---
         10.4.1.1   10.4.1.255   255     0

#### Meaning

Table 27 lists the show ip local pool command output fields.

Table 27: show ip local pool Output Fields

Field Name | Field Description
--- | ---
Pool | User-specified name of the address pool
High Thresh | High utilization threshold value
Abated Thresh | Abated utilization threshold value
Trap | Enable SNMP pool utilization traps: Y (yes) or N (no)
Aliases | Aliases for the local address pool
Begin | Starting IP address
End | Ending IP address
Free | Number of addresses available for use
In Use | Number of addresses currently in use

#### Related Documentation

- show ip local pool