# mpls traffic-eng attribute-flags

#### Syntax

mpls traffic-eng attribute-flags bitmask

no mpls traffic-eng attribute-flags

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies attributes for the interface for traffic engineering. The attributes are compared with tunnel affinity bits to determine links eligibility for the tunnel. The no version restores the default value, 0x0.

#### Options

- bitmask—Mask that sets the attributes, a value in the range 0x0–0xFFFFFFFF

#### Mode

Interface Configuration, Subinterface Configuration