# ip nat outside source static

#### Syntax

[ no ] ip nat outside source static globalIpAddress localIpAddress

[ no ] ip nat outside source static { tcp | udp } globalIpAddress globalPort localIpAddress localPort

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Translates the source address when routing a packet from the outside network to the inside network, and “ untranslates” the destination address when a packet travels from the inside network to the outside network. The no version removes the static translation and purges the associated translations from the translation table.

#### Options

- tcp—Indicates a TCP port
- udp—Indicates a UDP port
- globalIpAddress—Inside global address
- globalPort—Inside global TCP or UDP port
- localIpAddress—Inside local address
- localPort—Inside local TCP or UDP port

#### Mode

Global Configuration