# Monitoring All Routes in a BGP Community List

#### Purpose

Display routes that are permitted by a BGP community list.

#### Action

To display routes that are permitted by a BGP community list:

    host1#show ip community-list
    Community List 1:
      permit 752877569 (11488:1)
      permit 752877570 (11488:2)
      permit 752877571 (11488:3)
      permit 752877572 (11488:4)
    Community List 2:
      permit 4294967043 (local-as)

#### Meaning

Table 48 lists the show ip community-list command output fields.

Table 48: show ip community-list Output Fields

Field Name | Field Description
--- | ---
Community List 1 | Name of the community list
permit, deny | Condition statement for routes matching the condition