# show l2tp received-disconnect-cause-summary

#### Syntax

show l2tp received-disconnect-cause-summary [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays aggregate summary statistics for all information received by an LAC from an LNS about the cause of an L2TP session disconnection. The LAC receives this information from the LNS by means of a PPP Disconnect Cause Code attribute value pair (AVP) included in an L2TP Call-Disconnect-Notify (CDN) message.

#### Options

- filter—See Filtering show Commands

#### Mode

Privileged Exec