# subscriber disconnect

#### Syntax

[ no ] subscriber disconnect

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the E Series router to receive RADIUS-initiated disconnect messages from the RADIUS server. The no version restores the default, in which support for RADIUS-initiated disconnect messages is disabled on the router.

| Note: This command and the RADIUS dynamic-request server feature replace the radius disconnect client command, which has been deprecated and may be removed completely in a future release. The RADIUS Disconnect Configuration mode has also been deprecated.

#### Mode

RADIUS Configuration