# l2tp dial-out target

#### Syntax

l2tp dial-out target ipAddress ipAddressMask domainName profile profileName

no l2tp dial-out target ipAddress ipAddressMask

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines an L2TP dial-out target that enables the creation of a dial-out session. The no version removes the L2TP dial-out route or target.

#### Options

- ipAddress—IP address of the target
- ipAddressMask—IP address mask of the target
- domainName—Domain name to be used in the outgoing call Access-Request message
- profileName—Name of profile to be used in the creation of the interface stack

#### Mode

Global Configuration