# Assigning a Profile

To assign a profile to an interface, use the profile command from Interface mode.

profile

- Use to assign a profile to a PPP interface. The profile configuration is used to dynamically create an upper IP interface.
- Example
  host1(config-if)#interface atm 3/1.50 host1(config-if)#encapsulation ppp host1(config-if)#profile boston
- Use the no version to remove the assignment from the interface.
- See profile