# show ipv6 interface

#### Syntax

show ipv6 interface [ vrf vrfName ] [ brief | detail ]
[ interfaceType interfaceSpecifier ][ delta ] [ filter ]

To display summary information:

show ipv6 interface summary [ vrf vrfName ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Displays current state of all IPv6 interfaces or the IPv6 interfaces that you specify. The default is all interface types and all interfaces.

#### Options

- vrfName—Name of the VRF
- brief—Displays a brief summary of IPv6 status and configuration information
- detail—Shows a detailed display of IP status and configuration information
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- delta—Displays baselined statistics
- filter—See Filtering show Commands
- summary—Shows a detailed summary of IP status and configuration

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Monitoring the Policy Configuration of IPv6 Interfaces