# pppoe acName

#### Syntax

pppoe acName string

no pppoe acName

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Allows you to configure an access concentrator name for a PPPoE interface or profile. If no AC name is configured, the router name is used. The no version removes the access concentrator name.

#### Options

- string—AC name; 64 characters maximum

#### Mode

Interface Configuration, Profile Configuration