# mpls statistics next-hop

#### Syntax

[ no ] mpls statistics next-hop nextHopIndex

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Enables statistics collection for MPLS next hops. By default, statistics are enabled for next hops depending on the protocol that created the MPLS next hop. Statistics are not stored in NVS. The no version disables statistics collection.

#### Options

- nextHopIndex—Integer uniquely identifying a next hop; in the range 1–1048575

#### Mode

Global Configuration