# Monitoring BGP Aggregate Addresses

#### Purpose

Display information about aggregate addresses.

The show ip bgp aggregate-address and show bgp ipv6 aggregate-address commands display similar information.

#### Action

To display information about aggregate addresses:

    host1# show bgp ipv6 aggregate-address
    Prefix             AS set  Summ only  Attribute map   Advertise map     Suppress map
    3ffe::/48          No      No         None            None              None

#### Meaning

Table 27 lists the show bgp ipv6 aggregate-address command output fields.

Table 27: show bgp ipv6 aggregate-address Output Fields

Field Name | Field Description
--- | ---
Prefix | Prefix of the aggregate address
AS set | ASs in the AS-set path
Summary only | Displays a summary of aggregate address information
Attribute map | Displays the attribute maps for aggregate addresses
Advertise map | Displays the advertise maps for aggregate addresses
Suppress map | Displays the suppressed maps for the aggregate addresses

#### Related Documentation

- show bgp ipv6 aggregate-address
- show ip bgp aggregate-address