# ipv6-prefix-pool-name

#### Syntax

ipv6-prefix-pool-name poolName

no ipv6-prefix-pool-name

#### Release Information

Command introduced in JunosE Release 10.1.0.

#### Description

Specifies the IPv6 local prefix pool name to be used to delegate prefixes to the requesting router, when the RADIUS server does not return a pool name using the Framed-IPv6-Pool attribute. The no version removes the IPv6 local pool from the AAA domain map.

#### Options

- poolName—Name of the IPv6 local prefix pool to associate with the domain name; string of up to 16 alphanumeric characters

#### Mode

Domain Map Configuration