# baseline log

#### Syntax

baseline log [ last-reset | time [ utc ] month day year ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a baseline for logging events. To use the current system time, do not enter any options. There is no no version.

#### Options

- last-reset—Causes the router to display log messages generated since the last time the router was reset
- time—Time and date after which the router displays messages that are timestamped. To set the time, use the following syntax:

  Hour:Minute[:Second]—Current time in 24-hour format; seconds are optional

- utc—Indicates that the time entered is UTC (GMT) time; if you do not include this keyword, the router considers the time entered to be local time
- month—Name of the month in English
- day—Number of the day in the range 1–31
- year—Four-digit number of the year

#### Mode

Privileged Exec